##TPLHEADERSHORT##
##TPLBODY## ##TPLMENU## ##TPLMESSAGE##

Reader general settings
Description: |
Enable: |
Device: |
Group: | Valid values 1-64
Fallback: |
Fallback per caid: | ##FALLBACK_PERCAID##
##TPLREADERCONFIGLBWEIGHT##
Caid: |
Ident: | ##IDENTS##
CHID: | ##CHIDS##
Class: |
Local cards: | ##LOCALCARDS##
AU disabled: |
AU Provid: |
Ratelimit ECM: |
| ECM Unique: |
Ratelimittime: | ms
Additional ms to hold SRVID in slot: |
Cool down: |
delay: ms , | duration: ms. If used, you need to define both values
ECM not found limit: |
ECM whitelist: | ##ECMWHITELIST##
ECM HeaderWhitelist: | ##ECMHEADERWHITELIST##
Drop CWs with wrong checksum: |
Skip CWs checksum test: |
Skip CWs checksum test only for: | ##IGN_CHKSUM_ONLYFOR##
Emmcache: |
Saveemm: |
unknown | unique | shared | global
Blockemm: |
unknown | unique | shared | global
Block EMM by Len: |
##READERCONFIGSIDINS##
Reader specific settings for protocol ##PROTOCOL##
##READERDEPENDINGCONFIG## ##TPLREADEREDITCACHEEXAIOBIT##

##TPLFOOTER##